# 每种数据类型对应的床位数量

|  |  |
| --- | --- |
| 数据类型 | 床位数量 |
| Airway Leak Compensation Status | 1 |
| Alarm Status | 2 |
| Altura | 15 |
| Artificial Airway Compensation Status | 1 |
| Correlation Coefficient | 2 |
| Device Date | 2 |
| Device Name | 2 |
| Device Software Revision | 2 |
| Dynamic Compliance | 2 |
| Dynamic Compliance Over Last 20% Breath | 2 |
| FC | 12 |
| FR | 12 |
| Generic Message Code | 2 |
| Generic Message Text | 2 |
| Generic Respiration Rate | 2 |
| I:E Ratio | 1 |
| Inspiratory Flow Setting | 2 |
| Inspiratory Flow Trigger Setting | 2 |
| Inspiratory Pressure Setting | 1 |
| Inspiratory Time Setting | 2 |
| Inspired O2 (FiO2) | 2 |
| Inspired O2 (FiO2) Setting | 1 |
| Mandatory Respiration Rate Setting | 2 |
| Maximum Inspiratory Time Setting | 2 |
| Maximum Inspired Pressure Setting | 2 |
| Mean Airway Pressure | 2 |
| Minute Volume | 2 |
| PEEP/CPAP Setting | 1 |
| PNId | 12 |
| PNIm | 12 |
| PNIs | 12 |
| Peak Airway Pressure | 2 |
| Peak Expiratory Flow | 1 |
| Peak Inspiratory Flow | 1 |
| Percent of Minute Volume Leakage | 2 |
| Peso | 15 |
| Positive End Expiratory Pressure (PEEP) | 2 |
| Positive End Expiratory Pressure (PEEP) Setting | 2 |
| Pulso | 12 |
| Regional O2 Saturation (rSO2) | 2 |
| Resistance | 2 |
| SpO2 | 12 |
| Tidal Volume Setting | 2 |
| Time Constant | 2 |
| Ventilation Mode | 2 |
| rSO2 Area Under Curve (AUC) | 2 |
| rSO2 Baseline | 1 |
| tcpCO2 | 1 |
| tcpO2 | 1 |